Mạch công suất cho loa karaoke gia đình, công suất cao, dùng bình 12V, bảo vệ chống bụp loa không cần relay.
Thích hợp cho quý khách độ chế loa karaoke gia đình, đảm bảo không ù xì.
Mạch chịu được tải loa từ 2-4ôm.
công suất 145W, đánh căng được cặp loa 20 từ 80 (cặp loa nối song song).
Mạch tích hợp tăng áp, dùng cho bình 12v hoặc pin3s dòng yêu cầu từ 10A để cho công suất đạt đỉnh 
Sản phẩm được thiết kế và sản xuất bởi KHIEM AUDIO, quý khách có thắc mắc nào liên quan đến mạch Class D thì liên hệ shop hoặc qua zalo 0328375753.
Mỗi đơn hàng trước khi gói sẽ được quay video thử mạch, đảm bảo chất lượng hàng điện tử không có bất cứ sự cố nào.
Video test mạch công suất trên Youtube: https://youtu.be/DKIFBkUMmnc?si=mJwWcrxkF_Lw5tWN

<iframe class="video_youtube" src="https://www.youtube.com/embed/DKIFBkUMmnc" title="Chế mọi loa đơn giản chỉ dùng mạch công suất này" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

<iframe class="video_youtube" src="https://www.youtube.com/embed/Pqp8_MREt9E" title="Thử mạch công suất class d, xem dạng sóng có được như lời đồn??" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>
